1 - | Headlight fairing - rear-view mirrors

1 | Rearview mirror

2 | Screw

3 | Upper clamp

4 | Spring washer

5 | Bracket

6 | Nut

7 | Screw

8 | Headlight fairing

9 | Screw

10 | Windshield

11 | Nut

12 | Quick-release fastener

13 | Screw

14 | Washer

Parts catalogue

Instrument panel - headlight fairing
Handlebar and controls

Important
Bold reference numbers in this section identify parts not shown in the figures alongside the text, but which can be found in the exploded view diagram.
Removal of the rear-view mirrors
Undo the screws (2), remove the rearview mirrors (1) and recover the washers (4).
Refitting the rearview mirrors
Insert the mirror (1) in the clamp (3) and fit the screw (2) with the washer (4).
Tighten the screw (2) to the specified torque (Sect. C 3, Frame torque settings).
Removal of the headlight fairing (696+)
Counterhold the nuts (6) and unscrew the screws (9) from the headlight support and remove the headligt fairing (8) complete with the brackets (5).
To remove the brackets (5), undo the screws (7), taking care not to lose the quick-release fasteners (12).
Disassembly of the headlight fairing
If the windshield (10) needs replacing, unscrew the screws (13) taking care to recover the washers (14) and the nuts (11).
Remove the windshield (10).
Reassembly of the headlight fairing
Important
On refitting the headlight fairing, always refit the washers (14) in correspondence with the retaining screws (13) to avoid damaging the painted parts and the Plexiglas windshield (10).
Refitting is the reverse of removal; tighten the retaining screws (13) to the specified torque (Sect. C 3, Frame torque settings).
Refitting the headlight fairing (696+)
Fit the brackets (5) to the headlight support, fitting the screws (9) and nuts (6).
Counterhold the nuts (6) and tighten the screws (9) to the specified torque (Sect. C 3, Frame torque settings).
Refit the brackets (5), insert the screws (7) and tighten them to the specified torque (Sect. C 3, Frame torque settings).
Check that the quick-release fasteners (12) are inserted in the brackets on the headlight fairing.
Fit the headlight fairing, locating it on the headlight support and fit the screws (9) and nuts (6).
Tighten the screws (11) to the specified torque (Sect. C 3, Frame torque settings).