2 - | Fairings

1 | RH fuel tank cover

2 | LH fuel tank cover

3 | Front fuel tank cover

4 | Screw

5 | Rear fuel tank cover

6 | Spacer

7 | Screw

8 | Quick-release fastener

9 | Special screw

10 | Nylon washer

11 | Screw

12 | Screw

Parts catalogue

Fuel tank (cover)

Important
Bold reference numbers in this section identify parts not shown in the figures alongside the text, but which can be found in the exploded view diagram.
Removal of the fuel tank fairings
Remove the seat (Sect. E 3, Removal of the seat).
Unscrew the screws (7) and (12) securing the front tank cover (3) but do not remove the cover.
Undo the screws (4) and (11) eand remove the RH tank cover (1) and LH tank cover (2) releasing the tabs (A) from the slots (B) in the rear cover (5): recover the nylon washers (10).
Remove the front tank cover (3) and recover the spacers (6).
Unscrew the special screws (9) and remove the rear tank cover (5).
Refittings the fuel tank fairings
Locate the rear cover (5) on the fuel tank and secure it in place with the special screws (9).
Tighten the two upper special screws (9) to the specified torque (Sect. C 3, Frame torque settings).
Check that the four bushes (6) are installed on the front tank cover (3) with the larger diameter side facing upwards (as shown in the photo).
Locate the front tank cover (3) on the fuel tank.
Refit the right-hand tank cover (1), inserting the tabs (A) in the corresponding slots (B) in the rear cover (5).
Insert the screws (11) complete with the nylon washers (10) and screws (11) in the RH tank cover (1) and LH tank cover (2).
Insert the screws (7) and (12) in the front tank cover (3).
Tighten the screws (12) and (7) to the specified torque (Sect. C 3, Frame torque settings), starting with the front screw.
Tighten the screws (4) and (11) to the specified torque (Sect. C 3, Frame torque settings).
1