6 - | Protection and safety devices

Checking protection and safety device components
Checking the key switch
Disconnect the key switch (A) from the electrical system by opening its connection (see “Routing of wiring on frame”, Sect. P 1) and use a multimeter to check its internal connections as follows:
turn the key to OFF and connect a multimeter to contacts (1) and (4) to check electrical continuity (Sect. P 9, Using a multimeter to check the electrical systems concerning operation of the multimeter). The resistance reading should be near zero and, if present, the audible continuity signal should be emitted;
turn the key to ON and connect the multimeter to contacts (1) and (2) and then to (3) and (4) to check for electrical continuity. The resistance reading should be near zero and, if present, the audible continuity signal should be emitted;
turn the key to PARK and connect the multimeter to contacts (1) and (4) to check electrical continuity. The resistance reading should be near zero and, if present, the audible continuity signal should be emitted;
turn the key to LOCK and connect the multimeter to contacts (1) and (4) to check for electrical continuity. The resistance reading should be near zero and, if present, the continuity sound signal should be emitted.
Notes
The same checks can also be performed using the “DDS” tester (Sect. D 5, DDS tester).
Checking the sidestand switch
Remove the switch from the sidestand (Sect. H 5, Removal of the sidestand) and disconnect the main wiring harness connector from the switch (see “Routing of wiring on frame”, Sect. P 1).
Use an analogue or digital multimeter (Sect. P 9, Using a multimeter to check the electrical systems) to check operation of the switch (see table).
Notes
The same checks can also be performed using the “DDS” tester (Sect. D 5, DDS tester).

Pos. pin (A) | Consumers | Rating.
l - s | 0 | X
s - n | X | 0
Multimeter pos. | Green/ Green White | Green/ Yellow Black

0 = Open contact
X = Closed contact
Checking the fuses
The main fuse box (1) is located on the right-hand side of the frame.
The fuses are accessed by removing the cover, which shows the ampere ratings and mounting locations.
For ampere ratings, refer to the “Routing of wiring on frame”, Sect. P 1.
Important
Before replacing a damaged fuse with a new one of the same rating, identify the cause of the problem.
A blown fuse can be identified by the breakage of inner filament (A).
Important
Switch the ignition key to OFF before replacing a fuse to avoid possible short circuits.
Warning
Never use a fuse with a rating other than the specified value. Failure to observe this rule may damage the electric system or even cause fire.
As well as the fuses in the fuse box, the motorcycle has a 30 A fuse (1) located alongside the ECU to protect the electronic regulator (Sect. P 2, Rectifier-regulator).