5 - | Stands

1 | Sidestand

2 | Screw

3 | Bracket

4 | Screw

5 | Switch

6 | Inner spring

7 | Spring assembly

8 | Plate

9 | Pivot screw

10 | Nut

Parts catalogue

stands

Important
Bold reference numbers in this section identify parts not shown in the figures alongside the text, but which can be found in the exploded view diagram.
Removal of the sidestand
Unscrew and remove the screw (A) securing the LH footrest bracket (C) to the engine.
Loosen the screw (B) and release the LH footrest bracket (C) from the engine block.
Disconnect the wiring connector (5) of the sidestand switch (1) from the main wiring harness.
Unscrew the screw (2) securing the sidestand bracket (3) to the engine and remove the complete sidestand assembly.
Disassembly of the sidestand
Unscrew the retaining screw (4) and remove the sidestand switch (5).
Release the sidestand springs (6) and (7) from the connecting plate (8) of the sidestand bracket and remove them.
Unscrew the pivot screw (9) securing the sidestand to the bracket and remove the sidestand (1) and the nut (10).
Inspecting the sidestand
Fit the sidestand leg to the bracket and check that there is no excessive play. Ensure that the ends of the sidestand are not bent with respect to the shank. A stand which shows signs of cracking must be renewed immediately.
For details of how to test the switch (5), see Sect. P 6, Checking protection and safety device components.
Reassembly of the sidestand
Grease the sidestand leg (1) and fit it to the bracket (3). Secure it with the pivot screw (9) and the nut (10). Tighten the pivot screw (9) to the specified torque (Sect. C 3, Frame torque settings).
Position the sidestand return springs (6) and (7) and attach them to pivot plate (8) and stand leg (1).
Locate the switch (5) on the bracket so that is seats against the pivot screw (9).
Fit the retaining screw (4) and tighten to the specified torque (Sect. C 3, Frame torque settings).
Refitting the sidestand
Locate the sidestand bracket (3) between the engine and the LH footrest bracket (C) and fit the screw (2).
Connect the connector (5) of the sidestand switch to the main wiring harness.
For correct routing of the sidestand switch wiring, refer to the plates diagrams in Sect. P 1, Routing of wiring on frame.
Fit the screw (A) in the footrest bracket (C). Tighten the screws (2), (A) and (B) to the specified torque (Sect. C 3, Frame torque settings), in the indicated sequence.
H