4 - | Front mudguard

1 | Front mudguard

2 | Washer

3 | Rivet

4 | Clip

5 | Screw

6 | Nylon washer

Parts catalogue

Fuel tank (cover)

Important
Bold reference numbers in this section identify parts not shown in the figures alongside the text, but which can be found in the exploded view diagram.
Removal of the front mudguard
Disconnect the front brake hose (A) from the clip (4).
Remove the retaining screws (5) and recover the nylon washers (6).
Remove the front mudguard (1).
Notes
On USA versions, a reflector is mounted on the front mudguard (1).
Notes
The clip (4) is secured to the front mudguard by means of a shear rivet (3) with two washers (2).
Refitting the front mudguard
Warning
Do not use the motorcycle without the front mudguard fitted to avoid the risk of the brake pipes fouling the wheel on braking.
Apply threadlocker to the screws (5).
Position the front mudguard (1) and refit the retaining screws (5) with the washers (6).
Locate the front brake hose grommet (A) in the mudguard clip (4).
Tighten the screws (5) to the specified torque (Sect. C 3, Frame torque settings).