2 - | Symbols - Abbreviations - References

To allow quick and easy consultation, this manual uses graphic symbols to highlight situations in which maximum care is required, as well as practical advice or information. Pay attention to the meaning of the symbols since they serve to avoid repeating technical concepts or safety warnings throughout the text. The symbols should therefore be seen as an aid to memory. Please refer to this page whenever in doubt as to their meaning.
The terms right-hand (RH) and left-hand (LH) are used with reference to the motorcycle's direction of forward travel.
Warning
Failure to comply with these instructions may put you at risk, and could lead to severe injury or even death.
Important
Failure to follow the instructions in text marked with this symbol can lead to serious damage to the motorcycle and its components.
Notes
This symbol indicates additional useful information for the current operation.
Text references
(X)
References in bold type indicate a part that is not illustrated in the figures next to the text, but which can be found in the exploded views at the beginning of each chapter.
(X)
References in non-bold type indicate a part that is illustrated in the figures alongside the text.
Product specifications
Symbols in the diagram show the type of threadlocker, sealant or lubricant to be used at the points indicated. The table below shows the symbols used and the specifications of the various products.

Symbol | Specifications | Recommended product
|  | Engine oil (for specifications, see Sect. C 2, Fuel, lubricants and other fluids). | SHELL Advance Ultra 4
|  | DOT 4 special hydraulic brake fluid. | SHELL Advance Brake DOT 4
|  | SAE 80-90 gear oil or special products for chains with O‑rings. | SHELL Advance Chain or Advance Teflon Chain
|  | Anti-freeze (nitride, amine and phosphate free) 30 to 40% solution in water. | SHELL Advance coolant or Glycoshell
| GREASE A | Multipurpose, medium fibre, lithium grease. | SHELL Alvania R3
| GREASE B | Molybdenum disulphide grease, high mechanical stress and high temperature resistant. | SHELL Retinax HDX2
| GREASE C | Bearing/joint grease for parts subject to prolonged mechanical stress. Temperature range: -10 to 110 °C. | SHELL Retinax LX2
| GREASE D | Protective grease, with anti-corrosive and waterproofing properties. | SHELL Retinax HD2
| GREASE E | PANKL grease - PLB 05. |
| GREASE F | OPTIMOL grease - PASTE WHITE T. |
| LOCK 1 | Low-strength threadlocker. | Loctite 222
| LOCK 2 | Medium-strength threadlocker, compatible with oil. | Loctite 243
| LOCK 3 | High-strength threadlocker for threaded parts. | Loctite 270
| LOCK 4 | Flange sealant resistant to high mechanical stress and solvents. Resists high temperatures (up to 200 °C) and pressures up to 350 bar; fills gaps up to 0.4 mm. | Loctite 510
| LOCK 5 | Permanent adhesive for smooth or threaded cylindrical fasteners on mechanical parts. High resistance to mechanical stress and solvents. Temperature range: ‑55 to 175 °C. | Loctite 128455
| LOCK 6 | Pipe sealant for pipes and medium to large fasteners. For water and gases (except oxygen). Maximum filling capacity: 0.40 mm diameter clearance. | Loctite 577
| LOCK 7 | Speed bonder for rubber and plastics with elastomer charged ethylic base. | Loctite 480
| LOCK 8 | High-strength retaining compound for threaded parts, bearings, bushes, splines and keys. Temperature range: ‑55 to 150 °C. | Loctite 601
| LOCK 9 | Medium-strength threadlocker. | Loctite 406
| LOCK 10 | Product for metal parts to seal and lock cylindrical freely sliding or threaded couplings. Resistant to high mechanical stress and high temperature, excellent resistance to solvents and chemical attack. | Loctite 128443
| LOCK 11 | Medium-strength threadlocker. | Loctite 401
| LOCK 12 | Instant adhesive gel offering tensile/shear strength. | Loctite 454 gel
|  | DUCATI liquid gasket. | 942470014
|  | Exhaust pipe paste. Self-sealing paste, hardens when heated; resists temperatures exceeding 1000 °C. | Holts Firegum
|  | Spray used to protect electrical systems. Eliminates moisture and condensation and provides excellent corrosion resistance. Water repellent. | SHELL Advance Contact Cleaner
|  | Dry lubricant, polymerizing on contact with air. | Molycote D321R