2 - | Fuel, lubricants and other fluids

Fuel, lubricants and other fluids | Type | dm³ (litres)
Fuel tank, including a reserve of 3.5 dm3 (litres) | Unleaded fuel with an octane rating of at least 95-98 RON | 15
Sump and filter | SHELL Advance Ultra 4 | 3.1
Front/rear brake and clutch circuits | SHELL Advance Brake DOT 4 |
Protection for electrical contacts | SHELL Advance Contact Cleaner |
Front fork | SHELL Advance Fork 7.5 or DONAX TA | 538±2.5 cm3 (per leg)

Important
Do not use additives in fuel or lubricants.
Engine oil
A good quality engine oil has special properties. Use only a highly detergent engine oil with certified SE, SF or SG or higher service ratings as marked on the container.
Oil viscosity
SAE 15W-50
The other viscosity grades specified in the table can be used where the average ambient temperatures are within the limits shown.