3 - | Seat

1 | Seat

2 | Helmet lock cable

3 | Screw

4 | Tool tray

5 | Rubber

6 | Special screw

7 | Spacer

8 | Rubber mounting

9 | Elastic strap

10 | Seat cover

Parts catalogue

Seat

Important
Bold reference numbers in this section identify parts not shown in the figures alongside the text, but which can be found in the exploded view diagram.
Removal of the seat
Insert the key in the lock and simultaneously apply downward pressure in the area of the catch to release the pin.
Pull the seat backwards to release it from the front catches and remove it from the frame.
Disassembly of the seat
On the 696+ version, unscrew the two special screws (6) and slide off the seat cover (10).
Reassembly of the seat
Refit the seat cover (10) and tighten the special screws (6) to the specified torque (Sect. C 3, Frame torque settings).
Refitting the seat
To refit the seat, engage the front end of the seat base in the lugs (B) on the fuel tank, then push down on the rear end of the seat until you hear the latch click into place.
Removal of the tool tray
Remove the seat as described in the paragraph “Removal of the seat” in this section.
Uncsrew thew screws (3) and remove the tool tray (4).
Refitting the tool tray
Refit the tool tray (4), insert the screws (3) and tighten to the specified torque (Sect. C 3, Frame torque settings).
Refit the seat as described in this section in the paragraph “Refitting the seat”.