10 - | Evaporative emissions canister

1 | Screw

2 | Rubber

3 | Spacer

4 | LH air deflector

5 | Hose

6 | Plate

7 | Spacer

8 | Nut

9 | Evaporative emissions canister

10 | Hose clip

11 | Hose clip

12 | Filter/oil reservoir hose

13 | Hose clip

14 | Union/filter pipe

15 | Hose clip

16 | Hose

17 | Union

18 | Aluminium gasket

19 | Hose

20 | Breather hose

Parts catalogue

Fuel tank
Evaporative emissions canister

Important
Bold reference numbers in this section identify parts not shown in the figures alongside the text. Refer to the exploded view diagram.
Evaporative emissions canister system (USA versions only)
USA models are equipped with an additional system with an evaporative emissions canister that prevents fuel fumes from being discharged into the atmosphere.
The hose (12) is connected to the canister (9); when the fuel has been filtered, it is returned with the hose (14) to the intake manifolds via the hoses (16) and (14). Hoses (5) and (25) vent to the ground.
For correct positioning of the connection hoses consult the indications given below.
Removal of the evaporative emissions canister

Operation | Section reference
Raise the fuel tank | L 2, Removal of the fuel tank
Remove the tank covers | E 2, Removal of the fuel tank fairings

Disconnect the hose (12) connecting the evaporative emissions canister (9) to the fuel filler cap.
Release the hose (12) dfrom the drain hose (20) by removing the strap (A).
Loosen the hose clamps (15) connecting the canister (9) to the horizontal and vertical cylinders.
Undo the screws (B) and remove the LH air deflector (4), taking care to release the clutch hose (C) from the clips.
Remove the canister (9) from the LH deflector (4) by releasing it from the plate (6).
Refitting the evaporative emissions canister
To refit the canister, reverse the steps of the removal procedure, taking care to tighten the screws (B) to the specified torque (Sect. C 3, Frame torque settings).

Operation | Section reference
Refit the fuel tank | L 2, Refitting the fuel tank
Refit the tank covers | E 2, Refittings the fuel tank fairings

Positioning the hoses, clamps and canister filter
Positioning the hoses, clamps and canister filter
Positioning the hoses, clamps and canister filter