1.1 - | Technical specifications

General

| Reference | Technical specifications
Motorcycle dimensions | Total length | 2058 mm
| Total width | 784 mm
| Total height | 1012 mm
| Wheelbase | 1452 mm
| Height of handlebar grip from ground | 960 mm
| Seat height | 770 mm
| Front footrest height | 334 mm
| Rear footrest height | 507 mm
| Minimum ground clearance | 117 mm
| Dry weight in riding order without fuel: | 161 kg
| Weight without liquids and battery | 172 kg
| Weight fully laden | No greater than 390 kg
Frame | Type | Chromium-molybdenum tubular trellis frame
Subframe | Type | Cast aluminium
| Steering head angle | 22.8°
| Steering angle | 32°
| Trail | 87 mm
| Front wheel | Light alloy, with three spokes
| Front wheel size | MT 3.50x17"
| Front tyre size | 120/60 - ZR 17
| Rear wheel | Light alloy, three spokes with cush drive dampers
| Rear wheel size | MT 4.50x17"
| Rear tyre size | 160/60 - ZR 17
| Type of tyre | Radial tubeless tyres
| Front brake | Hydraulic with 2 calipers
| Rear brake | Hydraulic with 1 caliper
Engine | Type | Longitudinal 90º “L” twin cylinder, four-stroke.
| Bore | 88 mm
| Stroke | 57.2 mm
| Displacement | 696 cm3
| Compression ratio | 10.7±0.5:1
| Timing system | With toothed belt, single overhead camshaft, 2 valves per cylinder and 4 rocker arms.
| Lubrication system | Pump-forced
| Oil pump type | Gear pump with bypass valve
| Cooling system | Air-cooled
| Air filter | Filter element in the airbox
| Crankshaft type | One-piece

Colours

| Description | Code
| Ducati Anniversary Red Transparent Red frame with black wheels | 473.101 (PPG) 228.880 (PPG)
| Matt black Transparent Matt black frame with black wheels | 291.501 (PPG) 228.880 (PPG)
| Pearl white Transparent Matt black frame with black wheels | 490.019 (PPG) 228.880 (PPG)

Transmission

| Reference | Technical specifications
| Clutch | APTC wet multiplate |
| Clutch control | Hydraulic |
| Gearbox | 6 speed |
| Primary drive | 33/61
| Transmission ratio | 1.85
| Final drive | 15/45
| Gearbox type | With constant mesh spur gears, operated by a lever on the left side of the motorcycle
| Gear ratios |  |
| 1 st | 13/32 |
| 2 nd | 18/30 |
| 3 rd | 21/28 |
| 4 th | 23/26 |
| 5 th | 22/22 |
| 6 th | 26/24 |

Timing system/valves

| Reference | Adjusting clearance | Checking clearance
Timing diagram | With 1 mm valve clearance |  |
| Intake | Opening 18° B.T.D.C. Closing 60° A.B.D.C. |
| Exhaust system | Opening 53° B.B.D.C. Closing 23° A.T.D.C. |
| Intake valve diameter | 44 mm |
| Exhaust valve diameter | 38.5 mm |
Valve lift | With 0 mm valve clearance | Intake 11.20 mm Exhaust 10.80 mm |
| Opening rocker arm - intake | 0.10 to 0.15 mm | 0.05 to 0.15 mm
| Opening rocker arm - exhaust | 0.10 to 0.15 mm | 0.05 to 0.15 mm
| Closing rocker arm - intake | 0 to 0.05 mm | 0 to 0.20 mm
| Closing rocker arm - exhaust | 0 to 0.05 mm | 0 to 0.20 mm
Timing belt tensioning | DDS | 140±5 Hz (horizontal) 140±5 Hz (vertical) | 140±5 Hz (horizontal) 140±5 Hz (vertical)
| Minimum limit value | 70 Hz | 70 Hz

Cylinder/Piston

| Reference | Standard value | Service limit
Cylinder barrel | Max. bore ovality |  | 0.03 mm
| Max. bore taper |  | 0.03 mm
| Nominal diameter Class A Class B Class C | 88 mm 88.000 to 88.010 mm 88.010 to 88.020 mm 88.020 to 88.030 mm |
Piston-to-cylinder bore clearance |  | 0.025 to 0.045 mm |
Piston | Nominal diameter Class A Class B Class C | 88 mm 87.965 to 87.975 mm 87.975 to 87.985 mm 87.985 to 87.995 mm |
Connecting rod | Connecting-rod big-end diameter | 43.67 mm |
Big-end bearing-to-crankpin clearance |  | Ø 40.017 mm/0 to 0.016 mm |
Gudgeon pin–to-piston clearance |  | 0.015 to 0.058 mm |
| Nominal diameters | Ø 18 mm |
| Piston | Ø 18 mm/0.020 to 0.015 |
| Gudgeon pin | Ø 18 mm/0 to 0.004 |
Gudgeon pin-to-connecting rod clearance |  | 0.006 to 0.028 mm |
Cylinder compression | Standard Minimum Max. permissible difference | 11 to 13 bar | min 10 bar max 2 bar

Gearbox

| Reference | Standard value | Service limit
Gearbox shafts | Endfloat |  | 0.05 to 0.020 mm
Selector drum | Endfloat |  | 0.10 to 0.040 mm
Gear selector fork | Selector fork end thickness | 3.90 to 4.00 mm |
| Selector fork-to-gear clearance | 0.070 to 0.285 mm | 0.4 mm

Cooling system

| Reference | Technical specifications
Type | Air-cooled: heat dispersion through the extensive finning on the two cylinder barrel/head assemblies |

Front wheel

| Reference | Standard value | Service limit
Minimum tread depth | In the most worn part |  | 2 mm
Tyre pressure | Cold | 2.1 - 2.3 bar |
Axle runout | On 100 mm |  | 0.05 mm
Wheel rim runout | Radial |  | 1 mm (0.04 inc.)
| Lateral |  | 0.5 mm (0.02 inc.)

Front suspension

| Reference | Technical specifications
Type |  | SHOWA: 43 mm Ø upside-down hydraulic fork, non-adjustable
| Fork travel | 120 mm
Fork | Not adjustable. |
| Oil charge per leg | 538±2.5 cm3 (per leg)

Rear wheel

| Reference | Standard value | Service limit
Minimum tread depth | In the most worn part |  | 2 mm
Tyre pressure | Cold | 2.2 - 2.4 bar |
Swingarm pivot shaft runout | On 100 mm |  | 0.2 mm
Wheel rim runout | Radial |  | 1 mm (0.04 inc.)
| Lateral |  | 0.5 mm (0.02 inc.)
Chain | Make Type | D.I.D. 520 V6 |
| Dimensions | 5/8" x 1/4" |
| No. of links | 107 + 1 open |

Rear suspension

| Reference | Technical specifications
Type |  | SACHS: progressive monoshock with adjustable rebound, compression and spring preload.
Shock absorber | Stroke | 59.5 mm
| Hydraulic damping standard setting. Turn the adjusters fully clockwise until they stop, then turn them anticlockwise | Rebound: 8 clicks
| Standard preloaded spring length | 150±1 mm
| Wheel travel | 148 mm

Hydraulic brakes

| Reference | Standard value | Service limit
FRONT
Brake disc | Type | Drilled dual disc |
| Shim | 4 mm | 3.6 mm (min.)
| Flange material | Steel |
| Braking surface material | Steel |
| Diameter | 320 mm |
| Braking surface | 44 cm2 (per disc) |
Brake caliper | Make | Brembo |
| Type | P4.32K - 4 piston |
| Caliper cylinder diameter | 32 mm |
| Pad friction material | FERIT I/D 450-FF |
Brake master cylinder | Type | PS 15 |
| Master cylinder diameter | 15 mm |
REAR
Brake disc | Type | Drilled disc |
| Shim | 5 mm | 4.5 mm (min.)
| Material | Steel |
| Diameter | 245 mm |
| Braking surface | 25 cm2 |
Brake caliper | Make | Brembo |
| Type | P34C - 2 pistons |
| Caliper cylinder diameter | 34 mm |
| Pad friction material | FERIT I/D 450 FF |
Brake master cylinder | Type | PS11 |
| Master cylinder diameter | 11 mm |

Charging system/alternator

| Reference | Technical specifications
Battery | Voltage | 12 V
| Charge | 10 Ah
| Type | Sealed, maintenance free
Alternator | Capacity | 12 V - 480 W

Ignition system

| Reference | Technical specifications
Ignition | Type | Siemens electronic injection
Starting | Type | Electric starter motor, 12 V - 0.7 kW.
Spark plugs | Make and type | NGK DCPR8E (alternative CHAMPION RA6HC)
| Electrode gap | 0.7 to 0.8 mm

Fuel system

| Make | Type
| Unleaded fuel | 95-98 RON
| Throttle body | Ø 45 mm
| Injectors per cylinder | 1
| Holes per injector | 8

Injection system

| Make | Type
Electronic Control Unit | Siemens | M3C

Lights/instrument panel

| Reference | Technical specifications
Bulbs | Front headlight (low beam/high beam) | H7 (12 V - 55 W)
| Number plate light | C5W (12 V - 5 W)
| Side light | H6 (12 V - 6 W)
| Turn signal light | RY10W (12 V - 10 W)
| Tail light and brake light: | LED
Fuses | Regulator | 30 A
| Instrument panel | 5 A
| Injection | 20 A
| Key ON | 10 A
| ECU | 5 A
| Devices | 15 A
| High beam and low beam headlights, parking lights | 15 A
| Spare | 20 A
| Spare | 5 A