1 - | Wiring diagram

Wiring diagram

Key to wiring diagram

1 | Right-hand handlebar switch

2 | Key switch

3 | Horizontal cylinder spark plug

4 | Vertical cylinder spark plug

5 | Starter motor

6 | Starter contactor

7 | Battery

8 | Main fuse

9 | Regulator

10 | Alternator

11 | Rear right turn indicator

12 | Tail light

13 | Number plate light

14 | Rear left turn indicator

15 | Fuel tank

16 | Horizontal cylinder exhaust lambda sensor

17 | Injection relay

18 | Self-diagnosis/DDA

19 | Horizontal cylinder coil

20 | Vertical cylinder coil

21 | Headlight

22 | MAP sensor

23 | Horizontal cylinder injector

24 | Vertical cylinder injector

25 | Throttle position sensor

26 | Rpm/timing sensor

27 | Cylinder sensor

28 | Speed sensor

29 | Sidestand

30 | Horn

31 | Neutral switch

32 | Oil pressure switch

33 | Rear brake light switch

34 | ECU

35 | Fuses

36 | Clutch switch

37 | Front brake light switch

38 | Left-hand handlebar switch

39 | Transponder antenna

40 | Air temperature sensor

41 | Vertical cylinder exhaust lambda sensor

42 | Instrument panel

43 | Lights relay

44 | Front left turn indicator

45 | Front right turn indicator

Wiring colour codes
B Blue
Bk Black
Bn Brown
G Green
Gr Grey
Lb Light blue
O Orange
P Pink
R Red
V Violet
W White
Y Yellow
Key to fusebox

Position | Item | Rating
1 | Key ON | 10 A
2 | Side lights, high/low beam | 15 A
3 | Consumers | 15 A
4 | Instrument panel | 5 A
5 | Injection | 20 A
6 | ECU | 5 A
7 | Spare | 20 A
8 | Spare | 5 A

Routing of wiring on frame
The routing of the wiring has been optimised to ensure the minimum obstruction.
Each section is designed to prevent interference with parts that might damage wires or cause operating failures when riding. The plates on the following pages show the origins (“0” points) for correct re-routing of wiring and the locations of cable ties.
Each figure includes references to the plates showing the wiring routing or the item to which it must be connected.

Position |  | Description
1 | Plate A | Main wiring branch
2 | Plate B | Left-hand handlebar switch connector
3 | Plate B | Clutch connector
4 | Plate B | Clutch wire
5 | Plate B | Front brake light connector
6 | Plate B | Right-hand handlebar switch connector
7 | Plate B | Front brake light wire
8 | Plate C | Immobilizer antenna connector
9 | Plate C | Keyswitch connector
10 | Plate C | Immobilizer antenna wire
11 | Plate C | Key-switch
12 | Plate D | Front right turn indicator connector
13 | Plate D | Front left turn indicator connector
14 | Plate D | Headlight connector
15 | Plate D | Instrument panel connector
16 | Plate E | Vertical cylinder injector connector
17 | Plate E | Air/temperature sensor
18 | Plate E | Horizontal cylinder injector connector
19 | Plate F | Engine earth
20 | Plate F | Sidestand connector
21 | Plate F | Battery negative terminal
22 | Plate F | Sidestand wire
23 | Plate F | Alternator cable
24 | Plate G | Horn connector
25 | Plate H | Regulator/alternator connector
26 | Plate H | Regulator/main wiring harness connector
27 | Plate H | Voltage regulator
28 | Plate J | Potentiometer connector
29 | Plate K | Horizontal cylinder coil connector
30 | Plate L | Horizontal cylinder exhaust lambda sensor
31 | Plate L | Horizontal exhaust lambda sensor connector
32 | Plate L | Vertical exhaust lambda sensor connector
33 | Plate L | Fuel tank flange connector
34 | Plate L | Vertical cylinder exhaust lambda sensor
35 | Plate M | Data acquisition (DDA) connector
36 | Plate N | Rear wiring harness connector
37 | Plate N | Number plate light connector
38 | Plate N | Rear left turn indicator connector
39 | Plate N | Right rear turn indicator connector
40 | Plate N | Rear brake light connector
41 | Plate O | Fusebox
42 | Plate O | Throttle pressure/vacuum sensor
43 | Plate P | Contactor/battery positive terminal cable
44 | Plate P | Injection/lights relay
45 | Plate P | ECU connector
46 | Plate P | Vertical cylinder coil connector
47 | Plate P | Starter contactor connector
48 | Plate Q | Vertical cylinder temperature sensor
49 | Plate R | Pickup connector
50 | Plate R | Pickup sensor
51 | Plate P | Starter motor/contactor cable
52 | Plate S | Oil pressure switch connector
53 | Plate T | Neutral cable switch connection
54 | Plate U | Rear brake light sensor connector
55 | Plate U | Speed sensor connector
56 | Plate V | Speed sensor